{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Data","Soupis položek-","Soupis položek+"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data","index":0,"n_rows":192,"n_cols":15,"rows_kept":192,"cut":false,"hidden":false,"merged":[]}
[null,null,null,null,""]
[null,null,null,null,"název akce: Věznice H.Slavkov Velit.Bud-SILNOPR.ELE"]
[null,null,null,null,"popis: Věznice H.Slavkov Velit.Bud-SILNOPR.ELE"]
["p.č.","rok","č.ak.","kap.","č.položky","popis položky","mj.","množství","cena/mj.     ","cena celkem","Nh/mj.","Nh celkem","DPH","VKP","CKP"]
[1,2016,53,"DE",0,"R1-1.NP                        ozn.R1-1NP","ks",1,0,{"$f":"H5*I5","v":0},0,{"$f":"H5*K5","v":0},"S","*",171]
[2,2016,53,"DE",0,"R2-2.NP                        ozn.R2-2NP","ks",1,0,0,0,0,"S","*",182]
[3,2016,53,"DE",513386,"A-svítidlo záři ZC236/15opalHR T8/IP40/1235mm opal","ks",2,0,0,0,0,"Z","*",81]
[4,2016,53,"DE",513288,"B-svítidlo záři ZC254/15opal+DIM1-10V/HRT5/IP40/12","ks",6,0,0,0,0,"Z","*",82]
[null,2016,null,"DE",null,"10mm opal",null,null,null,0,0,0,null,"&"]
[5,2016,53,"DE",511261,"sví žár AuraD4 IN-22K7/072/G4 2xE27 IP41pr490 4080","ks",7,0,0,0,0,"Z","*",83]
[6,2016,53,"DE",529023,"svít žár ELEKTRA6 IN-172/L4  E27 IP65pr320mm 50053","ks",2,0,0,0,0,"Z","*",89]
[7,2016,53,"DE",721456,"skříň SR608/P_W 12x400A+6x160A rozpojovací/Vsvorky","ks",1,0,0,0,0,"Z","*",101]
[8,2016,53,"ME",171108,"vodič CY 6  /H07V-U/","m",50,0,0,0,0,"S","*",1]
[9,2016,53,"ME",171109,"vodič CY 10  /H07V-U/","m",100,0,0,0,0,"S","*",2]
[10,2016,53,"ME",171110,"vodič CY 16  /H07V-U/","m",60,0,0,0,0,"S","*",3]
[11,2016,53,"ME",101105,"kabel CYKY 3x1,5","m",1500,0,0,0,0,"S","*",4]
[12,2016,53,"ME",101305,"kabel CYKY 5x1,5","m",200,0,0,0,0,"S","*",5]
[13,2016,53,"ME",101106,"kabel CYKY 3x2,5","m",2850,0,0,0,0,"S","*",6]
[14,2016,53,"ME",101307,"kabel CYKY 5x4","m",20,0,0,0,0,"S","*",7]
[15,2016,53,"ME",101308,"kabel CYKY 5x6","m",45,0,0,0,0,"S","*",8]
[16,2016,53,"ME",101310,"kabel CYKY 5x16","m",18,0,0,0,0,"S","*",9]
[17,2016,53,"ME",101211,"kabel 1kV CYKY 4x25","m",22,0,0,0,0,"S","*",10]
[18,2016,53,"ME",199411,"svorkovnice typ EPS1  ekvipotenciální","ks",1,0,0,0,0,"S","*",31]
[19,2016,53,"ME",311117,"krabice univerz/rozvodka KU68-1903 vč.KO68 +S66","ks",60,0,0,0,0,"S","*",32]
[20,2016,53,"ME",311212,"krabice přístrojová KP68","ks",100,0,0,0,0,"S","*",33]
[21,2016,53,"ME",311213,"krabice přístrojová KPR68","ks",4,0,0,0,0,"S","*",34]
[22,2016,53,"ME",311222,"krabice přístrojová KP64/2","ks",76,0,0,0,0,"S","*",35]
[23,2016,53,"ME",311223,"krabice přístrojová KP64/3","ks",20,0,0,0,0,"S","*",36]
[24,2016,53,"ME",311224,"krabice přístrojová KP64/4","ks",54,0,0,0,0,"S","*",37]
[25,2016,53,"ME",311225,"krabice přístrojová KP64/5","ks",2,0,0,0,0,"S","*",38]
[26,2016,53,"ME",312911,"krabicová rozvodka ACIDUR 6455-11","ks",1,0,0,0,0,"S","*",39]
[27,2016,53,"ME","ABBJ3536N","SPINAC STIS PRESSTO ZAPUS.B/S","KS",1,0,0,0,0,"S","*",51]
[28,2016,53,"ME",410130,"SESTAVA  spínač 1pól Tango 10A/250Vstř řaz.1",null,20,0,0,0,0,null,"*",52]
[29,2016,53,"ME",409820,"spínač/strojek 10A/250Vstř 3558-A01340 řaz. 1,1So","ks",20,0,0,0,0,"S",null,52]
[30,2016,53,"ME",410101,"kryt spínače 1-duchý 3558A-A651 pro ř.1,6,7,1/0","ks",20,0,0,0,0,"S",null,52]
[31,2016,53,"ME",410153,"SESTAVA  přepín střídavý+N Tango 10A/250Vstř ř.6S",null,4,0,0,0,0,null,"*",53]
[32,2016,53,"ME",409823,"přep/strojek 10A/250Vstř 3558-A25342 ř.6,6So,6S +N","ks",4,0,{"$f":"H37*I37","v":0},0,{"$f":"H37*K37","v":0},"S",null,53]
[33,2016,53,"ME",409901,"doutnavka signalizační 3916-22221","ks",4,0,0,0,0,"S",null,53]
[34,2016,53,"ME",410103,"kryt spín 3558A-A653 pro ř.1So,6So,S,1/0So,S,7So","ks",4,0,0,0,0,"S",null,53]
[35,2016,53,"ME",410150,"SESTAVA  přepínač sériový Tango 10A/250Vstř řaz.5",null,18,0,0,0,0,null,"*",54]
[36,2016,53,"ME",409826,"přepínač/strojek 10A/250Vstř 3558-A05340 řazení 5","ks",18,0,0,0,0,"S",null,54]
[37,2016,53,"ME",410102,"kryt spínače dělený 3558A-A652 pro ř.5,6+6,1/0+1/0","ks",18,0,0,0,0,"S",null,54]
[38,2016,53,"ME",410162,"SESTAVA  ovladač zapín Tango 10A/250Vstř řaz.1/0S",null,32,0,0,0,0,null,"*",55]
[39,2016,53,"ME",409828,"ovladač/strojek 10A/250Vstř 3558-A91342 ř.1/0,S,So","ks",32,0,0,0,0,"S",null,55]
[40,2016,53,"ME",409901,"doutnavka signalizační 3916-22221","ks",32,0,0,0,0,"S",null,55]
[41,2016,53,"ME",410103,"kryt spín 3558A-A653 pro ř.1So,6So,S,1/0So,S,7So","ks",32,0,0,0,0,"S",null,55]
[42,2016,53,"ME",410170,"spínač automatic+snímač pohybu Tango 3299A-A12100","ks",1,0,0,0,0,"S","*",56]
[43,2016,53,"ME",420008,"zásuvka 16A/250Vstř Tango 5599A-A02357 bezŠr chrán","ks",30,0,0,0,0,"S","*",57]
[44,2016,53,"ME",420001,"zásuvka 16A/250Vstř Tango 5518A-A2349","ks",435,0,0,0,0,"S","*",58]
[45,2016,53,"ME",420091,"rámeček pro 1 přístroj Tango 3901A-B10","ks",100,0,0,0,0,"S","*",59]
[46,2016,53,"ME",420092,"rámeček pro 2 přístroje Tango 3901A-B20 vodorovný","ks",77,0,0,0,0,"S","*",60]
[47,2016,53,"ME",420093,"rámeček pro 3 přístroje Tango 3901A-B30 vodorovný","ks",20,0,0,0,0,"S","*",61]
[48,2016,53,"ME",420094,"rámeček pro 4 přístroje Tango 3901A-B40 vodorovný","ks",53,0,0,0,0,"S","*",62]
[49,2016,53,"ME",420095,"rámeček pro 5 přístrojů Tango 3901A-B50 vodorovný","ks",2,0,0,0,0,"S","*",63]
[50,2016,53,"ME",409018,"Detektor pohybu 180\"THEBEN lUXA 101-180,","ks",1,0,0,0,0,"S","*",64]
[51,2016,53,"ME","ELKO85951","RELE MULTIFUNKCNI SMR-H SUPER","KS",2,0,0,0,0,"S","*",65]
[52,2016,53,"ME",859518814,"RF Key/W bílá  Klíčenka RF, 4 kanály (tlačítka)","ks",1,0,0,0,0,"S","*",66]
[53,2016,53,"ME",859518814,"RFDAC-71B  Analogový RF aktor pro plynulou regulac","ks",1,0,0,0,0,"S","*",67]
[54,2016,53,"ME",859518814,"RFWB-20/G  Nástěnný RF ovladač, 2 kanály,","ks",1,0,0,0,0,"S","*",68]
[null,2016,null,"ME",null,"(komplet - bílá)",null,null,null,0,0,0,null,"&"]
[55,2016,53,"ME",592126,"zářivka lineární T8 pr26mm/L1200mm/G13 36W","ks",4,0,0,0,0,"Z",null,81]
[56,2016,53,"ME",592164,"zářivka lineární T5 HO pr16mm/L1149mm/G5 54W","ks",12,0,0,0,0,"Z",null,82]
[57,2016,53,"ME",40042,"C-AURA 2  IN-12DU52/042","ks",18,0,0,0,0,"Z","*",84]
[58,2016,53,"ME",219000000,"E-SVITIDLO LED VO PREMIUM TypII/TypIII. series","KS",1,0,0,0,0,"Z","*",85]
[null,2016,null,"ME",null,"P35,35W",null,null,null,0,0,0,null,"&"]
[59,2016,53,"ME",245039902,"Držák veř.osv.na zeď","ks",1,0,0,0,0,"Z","*",86]
[60,2016,53,"ME",859401050,"F-FIMB 849-Y39-C/2700 PETRA  T5 39W  IP20","ks",1,0,0,0,0,"Z","*",87]
[null,2016,null,"ME",null,"přisaz., trubicové int. svítidlo s lin. zářivkou,",null,null,null,0,0,0,null,"&"]
[61,2016,53,"ME",859558320,"N1-ANTARES AN-400  11W  IP42  přisaz., obdél.,","ks",12,0,{"$f":"H69*I69","v":0},0,{"$f":"H69*K69","v":0},"Z","*",88]
[null,2016,null,"ME",null,"nouzové 1h svítidlo, plast. čirý difuzor",null,null,null,0,0,0,null,"&"]
[62,2016,53,"ME",592354,"zářivka 1-paticová(E27) kompaktní 3U/26W","ks",36,0,0,0,0,"Z","*",90]
[63,2016,53,"ME",784233,"třmen Vsvorky 5845      do 240mm2","ks",18,0,0,0,0,"Z",null,101]
[64,2016,53,"ME",433163,"pojistková patrona PNA000(25-80A)gG","ks",6,0,0,0,0,"S","*",102]
[65,2016,53,"ME",433361,"pojistková patrona PNA2(35-63A)gG","ks",3,0,0,0,0,"S","*",103]
[66,2016,53,"ME",433362,"pojistková patrona PNA2(80-160A)gG","ks",6,0,0,0,0,"S","*",104]
[67,2016,53,"ME",433363,"pojistková patrona PNA2(200-250A)gG","ks",3,0,0,0,0,"S","*",105]
[68,2016,53,"ME",199513,"štítek kabelový 60x24mm velký","ks",6,0,0,0,0,"S","*",111]
[69,2016,53,"ME",101006,"kabel CYKY 2x2,5-REPRO","m",70,0,0,0,0,"S","*",161]
[70,2016,53,"ME",209403,"kabel U/UTP Cat.5e 4x2xAWG24 PVC plášť šedý","m",40,0,0,0,0,"S","*",162]
[71,2016,53,"ME",209487,"konektor komunikační RJ45-SD 8pol drát stíněný","ks",1,0,0,0,0,"S","*",163]
[72,2016,53,"ME",420086,"SESTAVA  zásuvka komunikační Tango 2xRJ45-8",null,1,0,0,0,0,"S","*",164]
[73,2016,53,"ME",420053,"kryt zásuvky komunikační Tango 5014A-A100","ks",1,0,0,0,0,"S",null,164]
[74,2016,53,"ME",420091,"rámeček pro 1 přístroj Tango 3901A-B10","ks",1,0,0,0,0,"S",null,164]
[75,2016,53,"ME",420204,"zásuvka komunik ModularJack RJ45-8Cat.5e 1208.10","ks",2,0,0,0,0,"S",null,164]
[76,2016,53,"ME",420212,"nosná maska pro 2xZásuvka ModularJack 5014A-B1018","ks",1,0,0,0,0,"S",null,164]
[77,2016,53,"ME","ELPRHDMI1","KABEL HDMI 1.4 10M GOLD ETH","KS",1,0,0,0,0,"S","*",165]
[78,2016,53,"ME",321112,"trubka ohebná PVC lpflex 2316E","m",25,0,0,0,0,"S","*",166]
[79,2016,53,"ME","ABBJ0230-","ZASUVKA REPRO STEREO BILA","KS",2,0,0,0,0,"S","*",168]
[80,2016,53,"ME",0,"stropní držák projektoru","ks",1,0,0,0,0,"S","*",169]
[81,2016,53,"ME",932,"ohnivzdorná přepážka s výplní(obecná položka)","m2",0.5,0,0,0,0,"S",null,41]
[82,2016,53,"MZ",46134,"beton B13,5","m3",0.05,0,0,0,0,"S",null,121]
[83,2016,53,"MZ",46141,"malta vápenocementová","kg",110,0,0,0,0,"S",null,121]
[84,2016,53,"MZ",46181,"cihla vápenopísková 24/11,5/7,1","ks",103,0,0,0,0,"S",null,121]
[85,2016,53,"MZ",46231,"plech FeZn tl.0,5mm","m2",0.63,0,0,0,0,"S",null,121]
[86,2016,53,"CE",210800006,"vodič Cu(-CY) pod omítkou do 1x16","m",50,0,0,0,0,"S",null,1]
[87,2016,53,"CE",210800006,"vodič Cu(-CY) pod omítkou do 1x16","m",100,0,0,0,0,"S",null,2]
[88,2016,53,"CE",210800006,"vodič Cu(-CY) pod omítkou do 1x16","m",60,0,0,0,0,"S",null,3]
[89,2016,53,"CE",210800103,"kabel Cu(-CYKY) pod omítkou do 2x4/3x2,5/5x1,5","m",1500,0,0,0,0,"S",null,4]
[90,2016,53,"CE",210800103,"kabel Cu(-CYKY) pod omítkou do 2x4/3x2,5/5x1,5","m",200,0,0,0,0,"S",null,5]
[91,2016,53,"CE",210800103,"kabel Cu(-CYKY) pod omítkou do 2x4/3x2,5/5x1,5","m",2850,0,0,0,0,"S",null,6]
[92,2016,53,"CE",210800112,"kabel Cu(-CYKY) pod omítkou do 5x6","m",20,0,{"$f":"H101*I101","v":0},0,{"$f":"H101*K101","v":0},"S",null,7]
[93,2016,53,"CE",210800112,"kabel Cu(-CYKY) pod omítkou do 5x6","m",45,0,0,0,0,"S",null,8]
[94,2016,53,"CE",210800114,"kabel Cu(-CYKY) pod omítkou do 5x16","m",18,0,0,0,0,"S",null,9]
[95,2016,53,"CE",210810101,"kabel Cu(-1kV CYKY) pevně uložený do 3x35/4x25","m",22,0,0,0,0,"S",null,10]
[96,2016,53,"CE",210100001,"ukončení v rozvaděči vč.zapojení vodiče do 2,5mm2","ks",300,0,0,0,0,"S","*",21]
[97,2016,53,"CE",210100002,"ukončení v rozvaděči vč.zapojení vodiče do 6mm2","ks",12,0,0,0,0,"S","*",22]
[98,2016,53,"CE",210100003,"ukončení v rozvaděči vč.zapojení vodiče do 16mm2","ks",20,0,0,0,0,"S","*",23]
[99,2016,53,"CE",210100004,"ukončení v rozvaděči vč.zapojení vodiče do 25mm2","ks",10,0,0,0,0,"S","*",24]
[100,2016,53,"CE",210100007,"ukončení v rozvaděči vč.zapojení vodiče do 70mm2","ks",1,0,0,0,0,"S","*",25]
[101,2016,53,"CE",210100003,"ukončení v rozvaděči vč.zapojení vodiče do 16mm2","ks",12,0,0,0,0,"S","*",106]
[102,2016,53,"CE",210100004,"ukončení v rozvaděči vč.zapojení vodiče do 25mm2","ks",4,0,0,0,0,"S","*",107]
[103,2016,53,"CE",210100007,"ukončení v rozvaděči vč.zapojení vodiče do 70mm2","ks",1,0,0,0,0,"S","*",108]
[104,2016,53,"CE",210100009,"ukončení v rozvaděči vč.zapojení vodiče do 120mm2","ks",4,0,0,0,0,"S","*",109]
[105,2016,53,"CE",210100012,"ukončení v rozvaděči vč.zapojení vodiče do 240mm2","ks",3,0,0,0,0,"S","*",110]
[106,2016,53,"CE",210950101,"označovací štítek na kabel","ks",110,0,0,0,0,"S",null,111]
[107,2016,53,"CE",210192562,"ochranná svorkovnice(nulový můstek)vč.zapoj.do 63A","ks",1,0,0,0,0,"S",null,31]
[108,2016,53,"CE",210010321,"krabicová rozvodka vč.svorkovn.a zapojení(-KR68)","ks",60,0,0,0,0,"S",null,32]
[109,2016,53,"CE",210010301,"krabice přístrojová bez zapojení","ks",100,0,0,0,0,"S",null,33]
[110,2016,53,"CE",210010301,"krabice přístrojová bez zapojení","ks",4,0,0,0,0,"S",null,34]
[111,2016,53,"CE",210010301,"krabice přístrojová bez zapojení","ks",76,0,0,0,0,"S",null,35]
[112,2016,53,"CE",210010301,"krabice přístrojová bez zapojení","ks",20,0,0,0,0,"S",null,36]
[113,2016,53,"CE",210010301,"krabice přístrojová bez zapojení","ks",54,0,0,0,0,"S",null,37]
[114,2016,53,"CE",210010301,"krabice přístrojová bez zapojení","ks",2,0,0,0,0,"S",null,38]
[115,2016,53,"CE",210010351,"krabicová rozvodka vč.ukonč.a zapojení (-6455/11)","ks",1,0,0,0,0,"S",null,39]
[116,2016,53,"CE",210110081,"spínač 3pól/25A/400V(sporák přípoj)vč.zapoj nástěn","ks",1,0,0,0,0,"S",null,51]
[117,2016,53,"CE",210110041,"spínač zapuštěný vč.zapojení 1pólový/řazení 1","ks",20,0,0,0,0,"S",null,52]
[118,2016,53,"CE",210110045,"přepínač zapuštěný vč.zapojení střídavý/řazení 6","ks",4,0,0,0,0,"S",null,53]
[119,2016,53,"CE",210110043,"přepínač zapuštěný vč.zapojení sériový/řazení 5-5A","ks",18,0,0,0,0,"S",null,54]
[120,2016,53,"CE",210110064,"ovladač zapuštěný vč.zapojení tlačítkový/ř.1/0 S","ks",32,0,0,0,0,"S",null,55]
[121,2016,53,"CE",210110091,"spínač zapuštěný vč.zapojení s plynulou regulací","ks",1,0,0,0,0,"S",null,56]
[122,2016,53,"CE",210111012,"zásuvka domovní zapuštěná vč.zapojení průběžně","ks",30,0,0,0,0,"S",null,57]
[123,2016,53,"CE",210111012,"zásuvka domovní zapuštěná vč.zapojení průběžně","ks",435,0,0,0,0,"S",null,58]
[124,2016,53,"CE",210110091,"spínač zapuštěný vč.zapojení s plynulou regulací","ks",1,0,{"$f":"H133*I133","v":0},0,{"$f":"H133*K133","v":0},"S",null,64]
[125,2016,53,"CE",210150481,"relé časové vč.zapojení(-TX)","ks",2,0,0,0,0,"S",null,65]
[126,2016,53,"CE",210110064,"ovladač zapuštěný vč.zapojení tlačítkový/ř.1/0 S","ks",1,0,0,0,0,"S",null,67]
[127,2016,53,"CE",210110027,"spínač nástěnný od IP.2 vč.zapojení 3pólový/25A","ks",1,0,0,0,0,"S",null,68]
[128,2016,53,"CE",210201002,"svítidlo zářivkové bytové stropní/2 zdroje","ks",2,0,0,0,0,"S",null,81]
[129,2016,53,"CE",210201002,"svítidlo zářivkové bytové stropní/2 zdroje","ks",6,0,0,0,0,"S",null,82]
[130,2016,53,"CE",210200012,"svítidlo žárovkové bytové stropní/více zdrojů","ks",7,0,0,0,0,"S",null,83]
[131,2016,53,"CE",210200011,"svítidlo žárovkové bytové stropní/1 zdroj","ks",18,0,0,0,0,"S",null,84]
[132,2016,53,"CE",210202103,"E-svítidlo výbojkové venkovní na výložník","ks",1,0,0,0,0,"S",null,85]
[133,2016,53,"CE",210202103,"svítidlo výbojkové venkovní na výložník","ks",1,0,0,0,0,"S",null,86]
[134,2016,53,"CE",210201041,"svítidlo zářivkové nástěnné kompaktní","ks",1,0,0,0,0,"S",null,87]
[135,2016,53,"CE",210201041,"svítidlo zářivkové nástěnné kompaktní","ks",12,0,0,0,0,"S",null,88]
[136,2016,53,"CE",210200131,"svítidlo žárovkové průmyslové nástěnné","ks",2,0,0,0,0,"S",null,89]
[137,2016,53,"CE",210201002,"STÁVAJÍCÍ svítidlo zářivkové stropní/2 zdroje","ks",50,0,0,0,0,"S","*",91]
[138,2016,53,"CE",210200041,"STÁVAJÍCÍ svítidlo žárovkové nástěnné/1 zdroj","ks",8,0,0,0,0,"S","*",92]
[139,2016,53,"CE",210191513,"kabelová skříň plast SPR2-SPR5 /osazení bez ukonč.","ks",1,0,0,0,0,"S",null,101]
[140,2016,53,"CE",210120103,"patrona nožové pojistky do 630A","ks",6,0,0,0,0,"S",null,102]
[141,2016,53,"CE",210120103,"patrona nožové pojistky do 630A","ks",3,0,0,0,0,"S",null,103]
[142,2016,53,"CE",210120103,"patrona nožové pojistky do 630A","ks",6,0,0,0,0,"S",null,104]
[143,2016,53,"CE",210120103,"patrona nožové pojistky do 630A","ks",3,0,0,0,0,"S",null,105]
[144,2016,53,"CE",210190002,"R1-rozvodnice do hmotnosti 50kg","ks",1,0,0,0,0,"S",null,182]
[145,2016,53,"CE",210190002,"R2-rozvodnice do hmotnosti 50kg","ks",1,0,0,0,0,"S","*",183]
[146,2016,53,"CE",210800103,"kabel Cu(-CYKY) pod omítkou do 2x4/3x2,5/5x1,5","m",70,0,0,0,0,"S",null,161]
[147,2016,53,"CE",210950341,"vodič/kabel v trubce jednotková hmotnost do 0,4kg","m",40,0,0,0,0,"S",null,162]
[148,2016,53,"CE",210111602,"zástrčka komunikační/konektor vč.zapojení 8pol","ks",1,0,0,0,0,"S",null,163]
[149,2016,53,"CE",210111312,"zásuvka domovní sdělovací 2násobná vč.zapojení","ks",1,0,0,0,0,"S",null,164]
[150,2016,53,"CE",210010002,"trubka plast ohebná,pod omítkou,typ 2316/pr.16","m",25,0,0,0,0,"S",null,166]
[151,2016,53,"CE",210020653,"nosná konstrukce přístroje do 50kg","ks",1,0,0,0,0,"S",null,169]
[152,2016,53,"CE",210200131,"svítidlo žárovkové průmyslové nástěnné","ks",4,0,0,0,0,"S",null,170]
[153,2016,53,"CE",210020921,"ohnivzdorná přepážka s výplní ve stěně tl.15cm","m2",0.5,0,0,0,0,"S","*",41]
[154,2016,53,"CZ",460270002,"OPRAVA zděný pilíř pro skříň SR","ks",1,0,0,0,0,"S","*",121]
[155,2016,53,"ON",219001233,"vybour.otvoru ve zdi/cihla/ do 0,09m2/tl.do 0,45m","ks",2,0,0,0,0,"S","*",122]
[156,2016,53,"ON",219003224,"zazdívka otvoru ve zdivu/cihla/do 0,09m2/tl.0,45m","ks",2,0,{"$f":"H165*I165","v":0},0,{"$f":"H165*K165","v":0},"S","*",123]
[157,2016,53,"ON",219001221,"vybour.otvoru ve zdi/cihla/ do 0,022m2/tl.do 0,15m","ks",40,0,0,0,0,"S","*",124]
[158,2016,53,"ON",219003212,"zazdívka otvoru ve zdivu/cihla/do 0,022m2/tl.0,15m","ks",40,0,0,0,0,"S","*",125]
[159,2016,53,"ON",219002271,"R1-vysekání výklenku/zeď cihla/ plocha od 0,25m2","m3",0.72,0,0,0,0,"S","*",126]
[160,2016,53,"ON",219003245,"R1-zazdívka otvoru ve zdivu/cihla/od 0,25m2 do 1,0","m3",0.72,0,0,0,0,"S","*",127]
[161,2016,53,"ON",219002271,"R2-vysekání výklenku/zeď cihla/ plocha od 0,25m2","m3",0.72,0,0,0,0,"S","*",128]
[162,2016,53,"ON",219003245,"R2-zazdívka otvoru ve zdivu/cihla/od 0,25m2 do 1,0","m3",0.72,0,0,0,0,"S","*",129]
[163,2016,53,"ON",219002611,"vysekání rýhy/zeď cihla/ hl.do 30mm/š.do 30mm","m",150,0,0,0,0,"S","*",130]
[164,2016,53,"ON",219003691,"omítka hladká rýhy ve stěně do 30mm vč.malty MV","m",150,0,0,0,0,"S","*",131]
[165,2016,53,"ON",219002631,"vysekání rýhy/zeď cihla/ hl.do 70mm/š.do 70mm","m",250,0,0,0,0,"S","*",132]
[166,2016,53,"ON",219003692,"omítka hladká rýhy ve stěně do 70mm vč.malty MV","m",250,0,0,0,0,"S","*",133]
[167,2016,53,"ON",219002641,"vysekání rýhy/zeď cihla/ hl.do 100mm/š.do 100mm","m",400,0,0,0,0,"S","*",134]
[168,2016,53,"ON",219003693,"omítka hladká rýhy ve stěně do 100mm vč.malty MV","m",400,0,0,0,0,"S","*",135]
[169,2016,53,"ON",219002661,"vysekání rýhy/zeď cihla/ hl.do 300mm/š.do 200mm","m",120,0,0,0,0,"S","*",136]
[170,2016,53,"ON",219003697,"omítka hladká rýhy ve stěně do 300mm vč.malty MV","m",120,0,0,0,0,"S","*",137]
[171,2016,53,"ON",219002671,"vysekání rýhy/zeď cihla/pod strop hl.30mm/š.30mm","m",220,0,0,0,0,"S","*",138]
[172,2016,53,"ON",219003591,"omítka hladká rýhy ve stropě do 30mm vč.malty MV","m",220,0,0,0,0,"S","*",139]
[173,2016,53,"ON",219990011,"Demontáže","hod",300,0,0,0,0,"S","*",191]
[174,2016,53,"ON",219990011,"Stěhování nábytku,úklid-25xkancel.á6hod.","hod",150,0,0,0,0,"S","*",192]
[175,2016,53,"ON",218009001,"poplatek za recyklaci svítidla","ks",2,0,0,0,0,"Z",null,81]
[176,2016,53,"ON",218009011,"poplatek za recyklaci světelného zdroje","ks",4,0,0,0,0,"Z",null,81]
[177,2016,53,"ON",218009001,"poplatek za recyklaci svítidla","ks",6,0,0,0,0,"Z",null,82]
[178,2016,53,"ON",218009011,"poplatek za recyklaci světelného zdroje","ks",12,0,0,0,0,"Z",null,82]
[179,2016,53,"ON",218009001,"poplatek za recyklaci svítidla","ks",1,0,0,0,0,"Z",null,85]
[180,2016,53,"ON",218009011,"poplatek za recyklaci světelného zdroje","ks",1,0,0,0,0,"Z",null,85]
[181,2016,53,"OP",1031,"držák pojistek D1PH","ks",1,0,0,0,0,"S",null,101]
[182,2016,53,"RE",217309013,"vypracování zprávy VR/cena akce do 1.000.000 kč","ks",2,0,0,0,0,"Z","*",193]
[null,null,null,null,null,"Celkem",null,null,null,{"$f":"SUM(J5:J191)","v":0},null,{"$f":"SUM(L5:L191)","v":0}]

{"sheet":"Soupis položek-","index":1,"n_rows":250,"n_cols":13,"rows_kept":250,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,""]
[null,"název akce: Věznice H.Slavkov Velit.Bud-SILNOPR.ELE"]
[null,"popis: Věznice H.Slavkov Velit.Bud-SILNOPR.ELE"]
[]
["Výkaz výměr"]
["p.č.","č.položky","popis položky","mj.","množství","cena/mj.     ","cena celkem","Nh/mj.","Nh celkem","DPH","VKP","TC","kap."]
["Dodávky zařízení"]
[1,0,"R1-1.NP                        ozn.R1-1NP","ks",1,0,{"$f":"E10*F10","v":0},0,{"$f":"E10*H10","v":0},"S","*",null,"DE"]
[2,0,"R2-2.NP                        ozn.R2-2NP","ks",1,0,{"$f":"E11*F11","v":0},0,{"$f":"E11*H11","v":0},"S","*",null,"DE"]
[null,null,"Osvětlení",null,null,null,null,null,null,null,null,"O","DE"]
[3,513386,"A-svítidlo záři ZC236/15opalHR T8/IP40/1235mm opal","ks",2,0,{"$f":"E13*F13","v":0},0,{"$f":"E13*H13","v":0},"Z","*","O","DE"]
[4,513288,"B-svítidlo záři ZC254/15opal+DIM1-10V/HRT5/IP40/12","ks",6,0,{"$f":"E14*F14","v":0},0,{"$f":"E14*H14","v":0},"Z","*","O","DE"]
[null,null,"10mm opal",null,null,null,{"$f":"E15*F15","v":0},0,{"$f":"E15*H15","v":0},null,"&","O","DE"]
[5,511261,"sví žár AuraD4 IN-22K7/072/G4 2xE27 IP41pr490 4080","ks",7,0,{"$f":"E16*F16","v":0},0,{"$f":"E16*H16","v":0},"Z","*","O","DE"]
[6,529023,"svít žár ELEKTRA6 IN-172/L4  E27 IP65pr320mm 50053","ks",2,0,{"$f":"E17*F17","v":0},0,{"$f":"E17*H17","v":0},"Z","*","O","DE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G13:G17)","v":0},null,null,null,null,null,null,"DE"]
[null,null,"Rozvaděče",null,null,null,null,null,null,null,null,"R","DE"]
[7,721456,"skříň SR608/P_W 12x400A+6x160A rozpojovací/Vsvorky","ks",1,0,{"$f":"E20*F20","v":0},0,{"$f":"E20*H20","v":0},"Z","*","R","DE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G20:G20)","v":0},null,null,null,null,null,null,"DE"]
[null,null," součet",null,null,null,{"$f":"SUM(G10:G21)","v":0},null,{"$f":"SUM(I10:I21)","v":0}]
["Materiál elektromontážní"]
[null,null,"Kabely",null,null,null,null,null,null,null,null,"K","ME"]
[8,171108,"vodič CY 6  /H07V-U/","m",50,0,{"$f":"E25*F25","v":0},0,{"$f":"E25*H25","v":0},"S","*","K","ME"]
[9,171109,"vodič CY 10  /H07V-U/","m",100,0,0,0,0,"S","*","K","ME"]
[10,171110,"vodič CY 16  /H07V-U/","m",60,0,0,0,0,"S","*","K","ME"]
[11,101105,"kabel CYKY 3x1,5","m",1500,0,0,0,0,"S","*","K","ME"]
[12,101305,"kabel CYKY 5x1,5","m",200,0,0,0,0,"S","*","K","ME"]
[13,101106,"kabel CYKY 3x2,5","m",2850,0,0,0,0,"S","*","K","ME"]
[14,101307,"kabel CYKY 5x4","m",20,0,0,0,0,"S","*","K","ME"]
[15,101308,"kabel CYKY 5x6","m",45,0,0,0,0,"S","*","K","ME"]
[16,101310,"kabel CYKY 5x16","m",18,0,0,0,0,"S","*","K","ME"]
[17,101211,"kabel 1kV CYKY 4x25","m",22,0,0,0,0,"S","*","K","ME"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G25:G34)","v":0},null,null,null,null,null,null,"ME"]
[null,null,"Materiál úložný",null,null,null,null,null,null,null,null,"M","ME"]
[18,199411,"svorkovnice typ EPS1  ekvipotenciální","ks",1,0,{"$f":"E37*F37","v":0},0,{"$f":"E37*H37","v":0},"S","*","M","ME"]
[19,311117,"krabice univerz/rozvodka KU68-1903 vč.KO68 +S66","ks",60,0,0,0,0,"S","*","M","ME"]
[20,311212,"krabice přístrojová KP68","ks",100,0,0,0,0,"S","*","M","ME"]
[21,311213,"krabice přístrojová KPR68","ks",4,0,0,0,0,"S","*","M","ME"]
[22,311222,"krabice přístrojová KP64/2","ks",76,0,0,0,0,"S","*","M","ME"]
[23,311223,"krabice přístrojová KP64/3","ks",20,0,0,0,0,"S","*","M","ME"]
[24,311224,"krabice přístrojová KP64/4","ks",54,0,0,0,0,"S","*","M","ME"]
[25,311225,"krabice přístrojová KP64/5","ks",2,0,0,0,0,"S","*","M","ME"]
[26,312911,"krabicová rozvodka ACIDUR 6455-11","ks",1,0,0,0,0,"S","*","M","ME"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G37:G45)","v":0},null,null,null,null,null,null,"ME"]
[null,null,"NNpřístroje",null,null,null,null,null,null,null,null,"N","ME"]
[27,"ABBJ3536N","SPINAC STIS PRESSTO ZAPUS.B/S","KS",1,0,{"$f":"E48*F48","v":0},0,{"$f":"E48*H48","v":0},"S","*","N","ME"]
[28,410130,"SESTAVA  spínač 1pól Tango 10A/250Vstř řaz.1",null,20,0,0,0,0,null,"*","N","ME"]
[29,409820,"spínač/strojek 10A/250Vstř 3558-A01340 řaz. 1,1So","ks",20,0,0,0,0,"S",null,"N","ME"]
[30,410101,"kryt spínače 1-duchý 3558A-A651 pro ř.1,6,7,1/0","ks",20,0,0,0,0,"S",null,"N","ME"]
[31,410153,"SESTAVA  přepín střídavý+N Tango 10A/250Vstř ř.6S",null,4,0,0,0,0,null,"*","N","ME"]
[32,409823,"přep/strojek 10A/250Vstř 3558-A25342 ř.6,6So,6S +N","ks",4,0,0,0,0,"S",null,"N","ME"]
[33,409901,"doutnavka signalizační 3916-22221","ks",4,0,0,0,0,"S",null,"N","ME"]
[34,410103,"kryt spín 3558A-A653 pro ř.1So,6So,S,1/0So,S,7So","ks",4,0,0,0,0,"S",null,"N","ME"]
[35,410150,"SESTAVA  přepínač sériový Tango 10A/250Vstř řaz.5",null,18,0,0,0,0,null,"*","N","ME"]
[36,409826,"přepínač/strojek 10A/250Vstř 3558-A05340 řazení 5","ks",18,0,0,0,0,"S",null,"N","ME"]
[37,410102,"kryt spínače dělený 3558A-A652 pro ř.5,6+6,1/0+1/0","ks",18,0,0,0,0,"S",null,"N","ME"]
[38,410162,"SESTAVA  ovladač zapín Tango 10A/250Vstř řaz.1/0S",null,32,0,0,0,0,null,"*","N","ME"]
[39,409828,"ovladač/strojek 10A/250Vstř 3558-A91342 ř.1/0,S,So","ks",32,0,0,0,0,"S",null,"N","ME"]
[40,409901,"doutnavka signalizační 3916-22221","ks",32,0,0,0,0,"S",null,"N","ME"]
[41,410103,"kryt spín 3558A-A653 pro ř.1So,6So,S,1/0So,S,7So","ks",32,0,0,0,0,"S",null,"N","ME"]
[42,410170,"spínač automatic+snímač pohybu Tango 3299A-A12100","ks",1,0,0,0,0,"S","*","N","ME"]
[43,420008,"zásuvka 16A/250Vstř Tango 5599A-A02357 bezŠr chrán","ks",30,0,0,0,0,"S","*","N","ME"]
[44,420001,"zásuvka 16A/250Vstř Tango 5518A-A2349","ks",435,0,0,0,0,"S","*","N","ME"]
[45,420091,"rámeček pro 1 přístroj Tango 3901A-B10","ks",100,0,0,0,0,"S","*","N","ME"]
[46,420092,"rámeček pro 2 přístroje Tango 3901A-B20 vodorovný","ks",77,0,0,0,0,"S","*","N","ME"]
[47,420093,"rámeček pro 3 přístroje Tango 3901A-B30 vodorovný","ks",20,0,0,0,0,"S","*","N","ME"]
[48,420094,"rámeček pro 4 přístroje Tango 3901A-B40 vodorovný","ks",53,0,0,0,0,"S","*","N","ME"]
[49,420095,"rámeček pro 5 přístrojů Tango 3901A-B50 vodorovný","ks",2,0,0,0,0,"S","*","N","ME"]
[50,409018,"Detektor pohybu 180\"THEBEN lUXA 101-180,","ks",1,0,0,0,0,"S","*","N","ME"]
[51,"ELKO85951","RELE MULTIFUNKCNI SMR-H SUPER","KS",2,0,0,0,0,"S","*","N","ME"]
[52,859518814,"RF Key/W bílá  Klíčenka RF, 4 kanály (tlačítka)","ks",1,0,0,0,0,"S","*","N","ME"]
[53,859518814,"RFDAC-71B  Analogový RF aktor pro plynulou regulac","ks",1,0,0,0,0,"S","*","N","ME"]
[54,859518814,"RFWB-20/G  Nástěnný RF ovladač, 2 kanály,","ks",1,0,0,0,0,"S","*","N","ME"]
[null,null,"(komplet - bílá)",null,null,null,0,0,0,null,"&","N","ME"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G48:G76)","v":0},null,null,null,null,null,null,"ME"]
[null,null,"Osvětlení",null,null,null,null,null,null,null,null,"O","ME"]
[55,592126,"zářivka lineární T8 pr26mm/L1200mm/G13 36W","ks",4,0,{"$f":"E79*F79","v":0},0,{"$f":"E79*H79","v":0},"Z",null,"O","ME"]
[56,592164,"zářivka lineární T5 HO pr16mm/L1149mm/G5 54W","ks",12,0,0,0,0,"Z",null,"O","ME"]
[57,40042,"C-AURA 2  IN-12DU52/042","ks",18,0,0,0,0,"Z","*","O","ME"]
[58,219000000,"E-SVITIDLO LED VO PREMIUM TypII/TypIII. series","KS",1,0,0,0,0,"Z","*","O","ME"]
[null,null,"P35,35W",null,null,null,0,0,0,null,"&","O","ME"]
[59,245039902,"Držák veř.osv.na zeď","ks",1,0,0,0,0,"Z","*","O","ME"]
[60,859401050,"F-FIMB 849-Y39-C/2700 PETRA  T5 39W  IP20","ks",1,0,0,0,0,"Z","*","O","ME"]
[null,null,"přisaz., trubicové int. svítidlo s lin. zářivkou,",null,null,null,0,0,0,null,"&","O","ME"]
[61,859558320,"N1-ANTARES AN-400  11W  IP42  přisaz., obdél.,","ks",12,0,0,0,0,"Z","*","O","ME"]
[null,null,"nouzové 1h svítidlo, plast. čirý difuzor",null,null,null,0,0,0,null,"&","O","ME"]
[62,592354,"zářivka 1-paticová(E27) kompaktní 3U/26W","ks",36,0,0,0,0,"Z","*","O","ME"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G79:G89)","v":0},null,null,null,null,null,null,"ME"]
[null,null,"Rozvaděče",null,null,null,null,null,null,null,null,"R","ME"]
[63,784233,"třmen Vsvorky 5845      do 240mm2","ks",18,0,{"$f":"E92*F92","v":0},0,{"$f":"E92*H92","v":0},"Z",null,"R","ME"]
[64,433163,"pojistková patrona PNA000(25-80A)gG","ks",6,0,0,0,0,"S","*","R","ME"]
[65,433361,"pojistková patrona PNA2(35-63A)gG","ks",3,0,0,0,0,"S","*","R","ME"]
[66,433362,"pojistková patrona PNA2(80-160A)gG","ks",6,0,0,0,0,"S","*","R","ME"]
[67,433363,"pojistková patrona PNA2(200-250A)gG","ks",3,0,0,0,0,"S","*","R","ME"]
[68,199513,"štítek kabelový 60x24mm velký","ks",6,0,0,0,0,"S","*","R","ME"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G92:G97)","v":0},null,null,null,null,null,null,"ME"]
[null,null,"Slaboproud-místn.205",null,null,null,null,null,null,null,null,"A","ME"]
[69,101006,"kabel CYKY 2x2,5-REPRO","m",70,0,{"$f":"E100*F100","v":0},0,{"$f":"E100*H100","v":0},"S","*","A","ME"]
[70,209403,"kabel U/UTP Cat.5e 4x2xAWG24 PVC plášť šedý","m",40,0,0,0,0,"S","*","A","ME"]
[71,209487,"konektor komunikační RJ45-SD 8pol drát stíněný","ks",1,0,0,0,0,"S","*","A","ME"]
[72,420086,"SESTAVA  zásuvka komunikační Tango 2xRJ45-8",null,1,0,0,0,0,"S","*","A","ME"]
[73,420053,"kryt zásuvky komunikační Tango 5014A-A100","ks",1,0,0,0,0,"S",null,"A","ME"]
[74,420091,"rámeček pro 1 přístroj Tango 3901A-B10","ks",1,0,0,0,0,"S",null,"A","ME"]
[75,420204,"zásuvka komunik ModularJack RJ45-8Cat.5e 1208.10","ks",2,0,0,0,0,"S",null,"A","ME"]
[76,420212,"nosná maska pro 2xZásuvka ModularJack 5014A-B1018","ks",1,0,0,0,0,"S",null,"A","ME"]
[77,"ELPRHDMI1","KABEL HDMI 1.4 10M GOLD ETH","KS",1,0,0,0,0,"S","*","A","ME"]
[78,321112,"trubka ohebná PVC lpflex 2316E","m",25,0,0,0,0,"S","*","A","ME"]
[79,"ABBJ0230-","ZASUVKA REPRO STEREO BILA","KS",2,0,0,0,0,"S","*","A","ME"]
[80,0,"stropní držák projektoru","ks",1,0,0,0,0,"S","*","A","ME"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G100:G111)","v":0},null,null,null,null,null,null,"ME"]
[null,null,"Protipožární zařízen",null,null,null,null,null,null,null,null,"B","ME"]
[81,932,"ohnivzdorná přepážka s výplní(obecná položka)","m2",0.5,0,{"$f":"E114*F114","v":0},0,{"$f":"E114*H114","v":0},"S",null,"B","ME"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G114:G114)","v":0},null,null,null,null,null,null,"ME"]
[null,null," součet",null,null,null,{"$f":"SUM(G24:G115)","v":0},null,{"$f":"SUM(I24:I115)","v":0}]
["Materiál zemní+stavební"]
[82,46134,"beton B13,5","m3",0.05,0,{"$f":"E118*F118","v":0},0,{"$f":"E118*H118","v":0},"S",null,null,"MZ"]
[83,46141,"malta vápenocementová","kg",110,0,{"$f":"E119*F119","v":0},0,{"$f":"E119*H119","v":0},"S",null,null,"MZ"]
[84,46181,"cihla vápenopísková 24/11,5/7,1","ks",103,0,{"$f":"E120*F120","v":0},0,{"$f":"E120*H120","v":0},"S",null,null,"MZ"]
[85,46231,"plech FeZn tl.0,5mm","m2",0.63,0,{"$f":"E121*F121","v":0},0,{"$f":"E121*H121","v":0},"S",null,null,"MZ"]
[null,null," součet",null,null,null,{"$f":"SUM(G118:G121)","v":0},null,{"$f":"SUM(I118:I121)","v":0}]
["Elektromontáže"]
[null,null,"Kabely",null,null,null,null,null,null,null,null,"K","CE"]
[86,210800006,"vodič Cu(-CY) pod omítkou do 1x16","m",50,0,{"$f":"E125*F125","v":0},0,{"$f":"E125*H125","v":0},"S",null,"K","CE"]
[87,210800006,"vodič Cu(-CY) pod omítkou do 1x16","m",100,0,0,0,0,"S",null,"K","CE"]
[88,210800006,"vodič Cu(-CY) pod omítkou do 1x16","m",60,0,0,0,0,"S",null,"K","CE"]
[89,210800103,"kabel Cu(-CYKY) pod omítkou do 2x4/3x2,5/5x1,5","m",1500,0,0,0,0,"S",null,"K","CE"]
[90,210800103,"kabel Cu(-CYKY) pod omítkou do 2x4/3x2,5/5x1,5","m",200,0,0,0,0,"S",null,"K","CE"]
[91,210800103,"kabel Cu(-CYKY) pod omítkou do 2x4/3x2,5/5x1,5","m",2850,0,0,0,0,"S",null,"K","CE"]
[92,210800112,"kabel Cu(-CYKY) pod omítkou do 5x6","m",20,0,0,0,0,"S",null,"K","CE"]
[93,210800112,"kabel Cu(-CYKY) pod omítkou do 5x6","m",45,0,0,0,0,"S",null,"K","CE"]
[94,210800114,"kabel Cu(-CYKY) pod omítkou do 5x16","m",18,0,0,0,0,"S",null,"K","CE"]
[95,210810101,"kabel Cu(-1kV CYKY) pevně uložený do 3x35/4x25","m",22,0,0,0,0,"S",null,"K","CE"]
[96,210100001,"ukončení v rozvaděči vč.zapojení vodiče do 2,5mm2","ks",300,0,0,0,0,"S","*","K","CE"]
[97,210100002,"ukončení v rozvaděči vč.zapojení vodiče do 6mm2","ks",12,0,0,0,0,"S","*","K","CE"]
[98,210100003,"ukončení v rozvaděči vč.zapojení vodiče do 16mm2","ks",20,0,0,0,0,"S","*","K","CE"]
[99,210100004,"ukončení v rozvaděči vč.zapojení vodiče do 25mm2","ks",10,0,0,0,0,"S","*","K","CE"]
[100,210100007,"ukončení v rozvaděči vč.zapojení vodiče do 70mm2","ks",1,0,0,0,0,"S","*","K","CE"]
[101,210100003,"ukončení v rozvaděči vč.zapojení vodiče do 16mm2","ks",12,0,0,0,0,"S","*","K","CE"]
[102,210100004,"ukončení v rozvaděči vč.zapojení vodiče do 25mm2","ks",4,0,0,0,0,"S","*","K","CE"]
[103,210100007,"ukončení v rozvaděči vč.zapojení vodiče do 70mm2","ks",1,0,0,0,0,"S","*","K","CE"]
[104,210100009,"ukončení v rozvaděči vč.zapojení vodiče do 120mm2","ks",4,0,0,0,0,"S","*","K","CE"]
[105,210100012,"ukončení v rozvaděči vč.zapojení vodiče do 240mm2","ks",3,0,0,0,0,"S","*","K","CE"]
[106,210950101,"označovací štítek na kabel","ks",110,0,0,0,0,"S",null,"K","CE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G125:G145)","v":0},null,null,null,null,null,null,"CE"]
[null,null,"Materiál úložný",null,null,null,null,null,null,null,null,"M","CE"]
[107,210192562,"ochranná svorkovnice(nulový můstek)vč.zapoj.do 63A","ks",1,0,{"$f":"E148*F148","v":0},0,{"$f":"E148*H148","v":0},"S",null,"M","CE"]
[108,210010321,"krabicová rozvodka vč.svorkovn.a zapojení(-KR68)","ks",60,0,0,0,0,"S",null,"M","CE"]
[109,210010301,"krabice přístrojová bez zapojení","ks",100,0,0,0,0,"S",null,"M","CE"]
[110,210010301,"krabice přístrojová bez zapojení","ks",4,0,0,0,0,"S",null,"M","CE"]
[111,210010301,"krabice přístrojová bez zapojení","ks",76,0,0,0,0,"S",null,"M","CE"]
[112,210010301,"krabice přístrojová bez zapojení","ks",20,0,0,0,0,"S",null,"M","CE"]
[113,210010301,"krabice přístrojová bez zapojení","ks",54,0,0,0,0,"S",null,"M","CE"]
[114,210010301,"krabice přístrojová bez zapojení","ks",2,0,0,0,0,"S",null,"M","CE"]
[115,210010351,"krabicová rozvodka vč.ukonč.a zapojení (-6455/11)","ks",1,0,0,0,0,"S",null,"M","CE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G148:G156)","v":0},null,null,null,null,null,null,"CE"]
[null,null,"NNpřístroje",null,null,null,null,null,null,null,null,"N","CE"]
[116,210110081,"spínač 3pól/25A/400V(sporák přípoj)vč.zapoj nástěn","ks",1,0,{"$f":"E159*F159","v":0},0,{"$f":"E159*H159","v":0},"S",null,"N","CE"]
[117,210110041,"spínač zapuštěný vč.zapojení 1pólový/řazení 1","ks",20,0,0,0,0,"S",null,"N","CE"]
[118,210110045,"přepínač zapuštěný vč.zapojení střídavý/řazení 6","ks",4,0,0,0,0,"S",null,"N","CE"]
[119,210110043,"přepínač zapuštěný vč.zapojení sériový/řazení 5-5A","ks",18,0,0,0,0,"S",null,"N","CE"]
[120,210110064,"ovladač zapuštěný vč.zapojení tlačítkový/ř.1/0 S","ks",32,0,0,0,0,"S",null,"N","CE"]
[121,210110091,"spínač zapuštěný vč.zapojení s plynulou regulací","ks",1,0,0,0,0,"S",null,"N","CE"]
[122,210111012,"zásuvka domovní zapuštěná vč.zapojení průběžně","ks",30,0,0,0,0,"S",null,"N","CE"]
[123,210111012,"zásuvka domovní zapuštěná vč.zapojení průběžně","ks",435,0,0,0,0,"S",null,"N","CE"]
[124,210110091,"spínač zapuštěný vč.zapojení s plynulou regulací","ks",1,0,0,0,0,"S",null,"N","CE"]
[125,210150481,"relé časové vč.zapojení(-TX)","ks",2,0,0,0,0,"S",null,"N","CE"]
[126,210110064,"ovladač zapuštěný vč.zapojení tlačítkový/ř.1/0 S","ks",1,0,0,0,0,"S",null,"N","CE"]
[127,210110027,"spínač nástěnný od IP.2 vč.zapojení 3pólový/25A","ks",1,0,0,0,0,"S",null,"N","CE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G159:G170)","v":0},null,null,null,null,null,null,"CE"]
[null,null,"Osvětlení",null,null,null,null,null,null,null,null,"O","CE"]
[128,210201002,"svítidlo zářivkové bytové stropní/2 zdroje","ks",2,0,{"$f":"E173*F173","v":0},0,{"$f":"E173*H173","v":0},"S",null,"O","CE"]
[129,210201002,"svítidlo zářivkové bytové stropní/2 zdroje","ks",6,0,0,0,0,"S",null,"O","CE"]
[130,210200012,"svítidlo žárovkové bytové stropní/více zdrojů","ks",7,0,0,0,0,"S",null,"O","CE"]
[131,210200011,"svítidlo žárovkové bytové stropní/1 zdroj","ks",18,0,0,0,0,"S",null,"O","CE"]
[132,210202103,"E-svítidlo výbojkové venkovní na výložník","ks",1,0,0,0,0,"S",null,"O","CE"]
[133,210202103,"svítidlo výbojkové venkovní na výložník","ks",1,0,0,0,0,"S",null,"O","CE"]
[134,210201041,"svítidlo zářivkové nástěnné kompaktní","ks",1,0,0,0,0,"S",null,"O","CE"]
[135,210201041,"svítidlo zářivkové nástěnné kompaktní","ks",12,0,0,0,0,"S",null,"O","CE"]
[136,210200131,"svítidlo žárovkové průmyslové nástěnné","ks",2,0,0,0,0,"S",null,"O","CE"]
[137,210201002,"STÁVAJÍCÍ svítidlo zářivkové stropní/2 zdroje","ks",50,0,0,0,0,"S","*","O","CE"]
[138,210200041,"STÁVAJÍCÍ svítidlo žárovkové nástěnné/1 zdroj","ks",8,0,0,0,0,"S","*","O","CE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G173:G183)","v":0},null,null,null,null,null,null,"CE"]
[null,null,"Rozvaděče",null,null,null,null,null,null,null,null,"R","CE"]
[139,210191513,"kabelová skříň plast SPR2-SPR5 /osazení bez ukonč.","ks",1,0,{"$f":"E186*F186","v":0},0,{"$f":"E186*H186","v":0},"S",null,"R","CE"]
[140,210120103,"patrona nožové pojistky do 630A","ks",6,0,0,0,0,"S",null,"R","CE"]
[141,210120103,"patrona nožové pojistky do 630A","ks",3,0,0,0,0,"S",null,"R","CE"]
[142,210120103,"patrona nožové pojistky do 630A","ks",6,0,0,0,0,"S",null,"R","CE"]
[143,210120103,"patrona nožové pojistky do 630A","ks",3,0,0,0,0,"S",null,"R","CE"]
[144,210190002,"R1-rozvodnice do hmotnosti 50kg","ks",1,0,0,0,0,"S",null,"R","CE"]
[145,210190002,"R2-rozvodnice do hmotnosti 50kg","ks",1,0,0,0,0,"S","*","R","CE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G186:G192)","v":0},null,null,null,null,null,null,"CE"]
[null,null,"Slaboproud-místn.205",null,null,null,null,null,null,null,null,"A","CE"]
[146,210800103,"kabel Cu(-CYKY) pod omítkou do 2x4/3x2,5/5x1,5","m",70,0,{"$f":"E195*F195","v":0},0,{"$f":"E195*H195","v":0},"S",null,"A","CE"]
[147,210950341,"vodič/kabel v trubce jednotková hmotnost do 0,4kg","m",40,0,0,0,0,"S",null,"A","CE"]
[148,210111602,"zástrčka komunikační/konektor vč.zapojení 8pol","ks",1,0,0,0,0,"S",null,"A","CE"]
[149,210111312,"zásuvka domovní sdělovací 2násobná vč.zapojení","ks",1,0,0,0,0,"S",null,"A","CE"]
[150,210010002,"trubka plast ohebná,pod omítkou,typ 2316/pr.16","m",25,0,0,0,0,"S",null,"A","CE"]
[151,210020653,"nosná konstrukce přístroje do 50kg","ks",1,0,0,0,0,"S",null,"A","CE"]
[152,210200131,"svítidlo žárovkové průmyslové nástěnné","ks",4,0,0,0,0,"S",null,"A","CE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G195:G201)","v":0},null,null,null,null,null,null,"CE"]
[null,null,"Protipožární zařízen",null,null,null,null,null,null,null,null,"B","CE"]
[153,210020921,"ohnivzdorná přepážka s výplní ve stěně tl.15cm","m2",0.5,0,{"$f":"E204*F204","v":0},0,{"$f":"E204*H204","v":0},"S","*","B","CE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G204:G204)","v":0},null,null,null,null,null,null,"CE"]
[null,null," součet",null,null,null,{"$f":"SUM(G124:G205)","v":0},null,{"$f":"SUM(I124:I205)","v":0}]
["Zemní práce"]
[154,460270002,"OPRAVA zděný pilíř pro skříň SR","ks",1,0,{"$f":"E208*F208","v":0},0,{"$f":"E208*H208","v":0},"S","*",null,"CZ"]
[null,null," součet",null,null,null,{"$f":"SUM(G208:G208)","v":0},null,{"$f":"SUM(I208:I208)","v":0}]
["Ostatní náklady"]
[155,219001233,"vybour.otvoru ve zdi/cihla/ do 0,09m2/tl.do 0,45m","ks",2,0,{"$f":"E211*F211","v":0},0,{"$f":"E211*H211","v":0},"S","*",null,"ON"]
[156,219003224,"zazdívka otvoru ve zdivu/cihla/do 0,09m2/tl.0,45m","ks",2,0,0,0,0,"S","*",null,"ON"]
[157,219001221,"vybour.otvoru ve zdi/cihla/ do 0,022m2/tl.do 0,15m","ks",40,0,0,0,0,"S","*",null,"ON"]
[158,219003212,"zazdívka otvoru ve zdivu/cihla/do 0,022m2/tl.0,15m","ks",40,0,0,0,0,"S","*",null,"ON"]
[159,219002271,"R1-vysekání výklenku/zeď cihla/ plocha od 0,25m2","m3",0.72,0,0,0,0,"S","*",null,"ON"]
[160,219003245,"R1-zazdívka otvoru ve zdivu/cihla/od 0,25m2 do 1,0","m3",0.72,0,0,0,0,"S","*",null,"ON"]
[161,219002271,"R2-vysekání výklenku/zeď cihla/ plocha od 0,25m2","m3",0.72,0,0,0,0,"S","*",null,"ON"]
[162,219003245,"R2-zazdívka otvoru ve zdivu/cihla/od 0,25m2 do 1,0","m3",0.72,0,0,0,0,"S","*",null,"ON"]
[163,219002611,"vysekání rýhy/zeď cihla/ hl.do 30mm/š.do 30mm","m",150,0,0,0,0,"S","*",null,"ON"]
[164,219003691,"omítka hladká rýhy ve stěně do 30mm vč.malty MV","m",150,0,0,0,0,"S","*",null,"ON"]
[165,219002631,"vysekání rýhy/zeď cihla/ hl.do 70mm/š.do 70mm","m",250,0,0,0,0,"S","*",null,"ON"]
[166,219003692,"omítka hladká rýhy ve stěně do 70mm vč.malty MV","m",250,0,0,0,0,"S","*",null,"ON"]
[167,219002641,"vysekání rýhy/zeď cihla/ hl.do 100mm/š.do 100mm","m",400,0,0,0,0,"S","*",null,"ON"]
[168,219003693,"omítka hladká rýhy ve stěně do 100mm vč.malty MV","m",400,0,0,0,0,"S","*",null,"ON"]
[169,219002661,"vysekání rýhy/zeď cihla/ hl.do 300mm/š.do 200mm","m",120,0,0,0,0,"S","*",null,"ON"]
[170,219003697,"omítka hladká rýhy ve stěně do 300mm vč.malty MV","m",120,0,0,0,0,"S","*",null,"ON"]
[171,219002671,"vysekání rýhy/zeď cihla/pod strop hl.30mm/š.30mm","m",220,0,0,0,0,"S","*",null,"ON"]
[172,219003591,"omítka hladká rýhy ve stropě do 30mm vč.malty MV","m",220,0,0,0,0,"S","*",null,"ON"]
[173,219990011,"Demontáže","hod",300,0,0,0,0,"S","*",null,"ON"]
[174,219990011,"Stěhování nábytku,úklid-25xkancel.á6hod.","hod",150,0,0,0,0,"S","*",null,"ON"]
[null,null,"Osvětlení",null,null,null,null,null,null,null,null,"O","ON"]
[175,218009001,"poplatek za recyklaci svítidla","ks",2,0,{"$f":"E232*F232","v":0},0,{"$f":"E232*H232","v":0},"Z",null,"O","ON"]
[176,218009011,"poplatek za recyklaci světelného zdroje","ks",4,0,0,0,0,"Z",null,"O","ON"]
[177,218009001,"poplatek za recyklaci svítidla","ks",6,0,0,0,0,"Z",null,"O","ON"]
[178,218009011,"poplatek za recyklaci světelného zdroje","ks",12,0,0,0,0,"Z",null,"O","ON"]
[179,218009001,"poplatek za recyklaci svítidla","ks",1,0,0,0,0,"Z",null,"O","ON"]
[180,218009011,"poplatek za recyklaci světelného zdroje","ks",1,0,0,0,0,"Z",null,"O","ON"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G232:G237)","v":0},null,null,null,null,null,null,"ON"]
[null,null," součet",null,null,null,{"$f":"SUM(G211:G238)","v":0},null,{"$f":"SUM(I211:I238)","v":0}]
["Ochranné a pracovní pomůcky"]
[null,null,"Rozvaděče",null,null,null,null,null,null,null,null,"R","OP"]
[181,1031,"držák pojistek D1PH","ks",1,0,{"$f":"E242*F242","v":0},0,{"$f":"E242*H242","v":0},"S",null,"R","OP"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G242:G242)","v":0},null,null,null,null,null,null,"OP"]
[null,null," součet",null,null,null,{"$f":"SUM(G241:G243)","v":0},null,{"$f":"SUM(I241:I243)","v":0}]
["Revize"]
[182,217309013,"vypracování zprávy VR/cena akce do 1.000.000 kč","ks",2,0,{"$f":"E246*F246","v":0},0,{"$f":"E246*H246","v":0},"Z","*",null,"RE"]
[null,null," součet",null,null,null,{"$f":"SUM(G246:G246)","v":0},null,{"$f":"SUM(I246:I246)","v":0}]
[]
["Datum: 8.11.2016"]
["Vypracoval:"]

{"sheet":"Soupis položek+","index":2,"n_rows":250,"n_cols":13,"rows_kept":250,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,""]
[null,"název akce: Věznice H.Slavkov Velit.Bud-SILNOPR.ELE"]
[null,"popis: Věznice H.Slavkov Velit.Bud-SILNOPR.ELE"]
[]
["Výkaz výměr"]
["p.č.","č.položky","popis položky","mj.","množství","cena/mj.     ","cena celkem","Nh/mj.","Nh celkem","DPH","VKP","TC","kap."]
["Dodávky zařízení"]
[1,0,"R1-1.NP                        ozn.R1-1NP","ks",1,0,{"$f":"E10*F10","v":0},0,{"$f":"E10*H10","v":0},"S","*",null,"DE"]
[2,0,"R2-2.NP                        ozn.R2-2NP","ks",1,0,{"$f":"E11*F11","v":0},0,{"$f":"E11*H11","v":0},"S","*",null,"DE"]
[null,null,"Osvětlení",null,null,null,null,null,null,null,null,"O","DE"]
[3,513386,"A-svítidlo záři ZC236/15opalHR T8/IP40/1235mm opal","ks",2,0,{"$f":"E13*F13","v":0},0,{"$f":"E13*H13","v":0},"Z","*","O","DE"]
[4,513288,"B-svítidlo záři ZC254/15opal+DIM1-10V/HRT5/IP40/12","ks",6,0,{"$f":"E14*F14","v":0},0,{"$f":"E14*H14","v":0},"Z","*","O","DE"]
[null,null,"10mm opal",null,null,null,{"$f":"E15*F15","v":0},0,{"$f":"E15*H15","v":0},null,"&","O","DE"]
[5,511261,"sví žár AuraD4 IN-22K7/072/G4 2xE27 IP41pr490 4080","ks",7,0,{"$f":"E16*F16","v":0},0,{"$f":"E16*H16","v":0},"Z","*","O","DE"]
[6,529023,"svít žár ELEKTRA6 IN-172/L4  E27 IP65pr320mm 50053","ks",2,0,{"$f":"E17*F17","v":0},0,{"$f":"E17*H17","v":0},"Z","*","O","DE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G13:G17)","v":0},null,null,null,null,null,null,"DE"]
[null,null,"Rozvaděče",null,null,null,null,null,null,null,null,"R","DE"]
[7,721456,"skříň SR608/P_W 12x400A+6x160A rozpojovací/Vsvorky","ks",1,0,{"$f":"E20*F20","v":0},0,{"$f":"E20*H20","v":0},"Z","*","R","DE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G20:G20)","v":0},null,null,null,null,null,null,"DE"]
[null,null,"součet",null,null,null,{"$f":"SUM(G10:G21)","v":0},null,{"$f":"SUM(I10:I21)","v":0}]
["Materiál elektromontážní"]
[null,null,"Kabely",null,null,null,null,null,null,null,null,"K","ME"]
[8,171108,"vodič CY 6  /H07V-U/","m",50,0,{"$f":"E25*F25","v":0},0,{"$f":"E25*H25","v":0},"S","*","K","ME"]
[9,171109,"vodič CY 10  /H07V-U/","m",100,0,0,0,0,"S","*","K","ME"]
[10,171110,"vodič CY 16  /H07V-U/","m",60,0,0,0,0,"S","*","K","ME"]
[11,101105,"kabel CYKY 3x1,5","m",1500,0,0,0,0,"S","*","K","ME"]
[12,101305,"kabel CYKY 5x1,5","m",200,0,0,0,0,"S","*","K","ME"]
[13,101106,"kabel CYKY 3x2,5","m",2850,0,0,0,0,"S","*","K","ME"]
[14,101307,"kabel CYKY 5x4","m",20,0,0,0,0,"S","*","K","ME"]
[15,101308,"kabel CYKY 5x6","m",45,0,0,0,0,"S","*","K","ME"]
[16,101310,"kabel CYKY 5x16","m",18,0,0,0,0,"S","*","K","ME"]
[17,101211,"kabel 1kV CYKY 4x25","m",22,0,0,0,0,"S","*","K","ME"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G25:G34)","v":0},null,null,null,null,null,null,"ME"]
[null,null,"Materiál úložný",null,null,null,null,null,null,null,null,"M","ME"]
[18,199411,"svorkovnice typ EPS1  ekvipotenciální","ks",1,0,{"$f":"E37*F37","v":0},0,{"$f":"E37*H37","v":0},"S","*","M","ME"]
[19,311117,"krabice univerz/rozvodka KU68-1903 vč.KO68 +S66","ks",60,0,0,0,0,"S","*","M","ME"]
[20,311212,"krabice přístrojová KP68","ks",100,0,0,0,0,"S","*","M","ME"]
[21,311213,"krabice přístrojová KPR68","ks",4,0,0,0,0,"S","*","M","ME"]
[22,311222,"krabice přístrojová KP64/2","ks",76,0,0,0,0,"S","*","M","ME"]
[23,311223,"krabice přístrojová KP64/3","ks",20,0,0,0,0,"S","*","M","ME"]
[24,311224,"krabice přístrojová KP64/4","ks",54,0,0,0,0,"S","*","M","ME"]
[25,311225,"krabice přístrojová KP64/5","ks",2,0,0,0,0,"S","*","M","ME"]
[26,312911,"krabicová rozvodka ACIDUR 6455-11","ks",1,0,0,0,0,"S","*","M","ME"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G37:G45)","v":0},null,null,null,null,null,null,"ME"]
[null,null,"NNpřístroje",null,null,null,null,null,null,null,null,"N","ME"]
[27,"ABBJ3536N","SPINAC STIS PRESSTO ZAPUS.B/S","KS",1,0,{"$f":"E48*F48","v":0},0,{"$f":"E48*H48","v":0},"S","*","N","ME"]
[28,410130,"SESTAVA  spínač 1pól Tango 10A/250Vstř řaz.1",null,20,0,0,0,0,null,"*","N","ME"]
[29,409820,"spínač/strojek 10A/250Vstř 3558-A01340 řaz. 1,1So","ks",20,0,0,0,0,"S",null,"N","ME"]
[30,410101,"kryt spínače 1-duchý 3558A-A651 pro ř.1,6,7,1/0","ks",20,0,0,0,0,"S",null,"N","ME"]
[31,410153,"SESTAVA  přepín střídavý+N Tango 10A/250Vstř ř.6S",null,4,0,0,0,0,null,"*","N","ME"]
[32,409823,"přep/strojek 10A/250Vstř 3558-A25342 ř.6,6So,6S +N","ks",4,0,0,0,0,"S",null,"N","ME"]
[33,409901,"doutnavka signalizační 3916-22221","ks",4,0,0,0,0,"S",null,"N","ME"]
[34,410103,"kryt spín 3558A-A653 pro ř.1So,6So,S,1/0So,S,7So","ks",4,0,0,0,0,"S",null,"N","ME"]
[35,410150,"SESTAVA  přepínač sériový Tango 10A/250Vstř řaz.5",null,18,0,0,0,0,null,"*","N","ME"]
[36,409826,"přepínač/strojek 10A/250Vstř 3558-A05340 řazení 5","ks",18,0,0,0,0,"S",null,"N","ME"]
[37,410102,"kryt spínače dělený 3558A-A652 pro ř.5,6+6,1/0+1/0","ks",18,0,0,0,0,"S",null,"N","ME"]
[38,410162,"SESTAVA  ovladač zapín Tango 10A/250Vstř řaz.1/0S",null,32,0,0,0,0,null,"*","N","ME"]
[39,409828,"ovladač/strojek 10A/250Vstř 3558-A91342 ř.1/0,S,So","ks",32,0,0,0,0,"S",null,"N","ME"]
[40,409901,"doutnavka signalizační 3916-22221","ks",32,0,0,0,0,"S",null,"N","ME"]
[41,410103,"kryt spín 3558A-A653 pro ř.1So,6So,S,1/0So,S,7So","ks",32,0,0,0,0,"S",null,"N","ME"]
[42,410170,"spínač automatic+snímač pohybu Tango 3299A-A12100","ks",1,0,0,0,0,"S","*","N","ME"]
[43,420008,"zásuvka 16A/250Vstř Tango 5599A-A02357 bezŠr chrán","ks",30,0,0,0,0,"S","*","N","ME"]
[44,420001,"zásuvka 16A/250Vstř Tango 5518A-A2349","ks",435,0,0,0,0,"S","*","N","ME"]
[45,420091,"rámeček pro 1 přístroj Tango 3901A-B10","ks",100,0,0,0,0,"S","*","N","ME"]
[46,420092,"rámeček pro 2 přístroje Tango 3901A-B20 vodorovný","ks",77,0,0,0,0,"S","*","N","ME"]
[47,420093,"rámeček pro 3 přístroje Tango 3901A-B30 vodorovný","ks",20,0,0,0,0,"S","*","N","ME"]
[48,420094,"rámeček pro 4 přístroje Tango 3901A-B40 vodorovný","ks",53,0,0,0,0,"S","*","N","ME"]
[49,420095,"rámeček pro 5 přístrojů Tango 3901A-B50 vodorovný","ks",2,0,0,0,0,"S","*","N","ME"]
[50,409018,"Detektor pohybu 180\"THEBEN lUXA 101-180,","ks",1,0,0,0,0,"S","*","N","ME"]
[51,"ELKO85951","RELE MULTIFUNKCNI SMR-H SUPER","KS",2,0,0,0,0,"S","*","N","ME"]
[52,859518814,"RF Key/W bílá  Klíčenka RF, 4 kanály (tlačítka)","ks",1,0,0,0,0,"S","*","N","ME"]
[53,859518814,"RFDAC-71B  Analogový RF aktor pro plynulou regulac","ks",1,0,0,0,0,"S","*","N","ME"]
[54,859518814,"RFWB-20/G  Nástěnný RF ovladač, 2 kanály,","ks",1,0,0,0,0,"S","*","N","ME"]
[null,null,"(komplet - bílá)",null,null,null,0,0,0,null,"&","N","ME"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G48:G76)","v":0},null,null,null,null,null,null,"ME"]
[null,null,"Osvětlení",null,null,null,null,null,null,null,null,"O","ME"]
[55,592126,"zářivka lineární T8 pr26mm/L1200mm/G13 36W","ks",4,0,{"$f":"E79*F79","v":0},0,{"$f":"E79*H79","v":0},"Z",null,"O","ME"]
[56,592164,"zářivka lineární T5 HO pr16mm/L1149mm/G5 54W","ks",12,0,0,0,0,"Z",null,"O","ME"]
[57,40042,"C-AURA 2  IN-12DU52/042","ks",18,0,0,0,0,"Z","*","O","ME"]
[58,219000000,"E-SVITIDLO LED VO PREMIUM TypII/TypIII. series","KS",1,0,0,0,0,"Z","*","O","ME"]
[null,null,"P35,35W",null,null,null,0,0,0,null,"&","O","ME"]
[59,245039902,"Držák veř.osv.na zeď","ks",1,0,0,0,0,"Z","*","O","ME"]
[60,859401050,"F-FIMB 849-Y39-C/2700 PETRA  T5 39W  IP20","ks",1,0,0,0,0,"Z","*","O","ME"]
[null,null,"přisaz., trubicové int. svítidlo s lin. zářivkou,",null,null,null,0,0,0,null,"&","O","ME"]
[61,859558320,"N1-ANTARES AN-400  11W  IP42  přisaz., obdél.,","ks",12,0,0,0,0,"Z","*","O","ME"]
[null,null,"nouzové 1h svítidlo, plast. čirý difuzor",null,null,null,0,0,0,null,"&","O","ME"]
[62,592354,"zářivka 1-paticová(E27) kompaktní 3U/26W","ks",36,0,0,0,0,"Z","*","O","ME"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G79:G89)","v":0},null,null,null,null,null,null,"ME"]
[null,null,"Rozvaděče",null,null,null,null,null,null,null,null,"R","ME"]
[63,784233,"třmen Vsvorky 5845      do 240mm2","ks",18,0,{"$f":"E92*F92","v":0},0,{"$f":"E92*H92","v":0},"Z",null,"R","ME"]
[64,433163,"pojistková patrona PNA000(25-80A)gG","ks",6,0,0,0,0,"S","*","R","ME"]
[65,433361,"pojistková patrona PNA2(35-63A)gG","ks",3,0,0,0,0,"S","*","R","ME"]
[66,433362,"pojistková patrona PNA2(80-160A)gG","ks",6,0,0,0,0,"S","*","R","ME"]
[67,433363,"pojistková patrona PNA2(200-250A)gG","ks",3,0,0,0,0,"S","*","R","ME"]
[68,199513,"štítek kabelový 60x24mm velký","ks",6,0,0,0,0,"S","*","R","ME"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G92:G97)","v":0},null,null,null,null,null,null,"ME"]
[null,null,"Slaboproud-místn.205",null,null,null,null,null,null,null,null,"A","ME"]
[69,101006,"kabel CYKY 2x2,5-REPRO","m",70,0,{"$f":"E100*F100","v":0},0,{"$f":"E100*H100","v":0},"S","*","A","ME"]
[70,209403,"kabel U/UTP Cat.5e 4x2xAWG24 PVC plášť šedý","m",40,0,0,0,0,"S","*","A","ME"]
[71,209487,"konektor komunikační RJ45-SD 8pol drát stíněný","ks",1,0,0,0,0,"S","*","A","ME"]
[72,420086,"SESTAVA  zásuvka komunikační Tango 2xRJ45-8",null,1,0,0,0,0,"S","*","A","ME"]
[73,420053,"kryt zásuvky komunikační Tango 5014A-A100","ks",1,0,0,0,0,"S",null,"A","ME"]
[74,420091,"rámeček pro 1 přístroj Tango 3901A-B10","ks",1,0,0,0,0,"S",null,"A","ME"]
[75,420204,"zásuvka komunik ModularJack RJ45-8Cat.5e 1208.10","ks",2,0,0,0,0,"S",null,"A","ME"]
[76,420212,"nosná maska pro 2xZásuvka ModularJack 5014A-B1018","ks",1,0,0,0,0,"S",null,"A","ME"]
[77,"ELPRHDMI1","KABEL HDMI 1.4 10M GOLD ETH","KS",1,0,0,0,0,"S","*","A","ME"]
[78,321112,"trubka ohebná PVC lpflex 2316E","m",25,0,0,0,0,"S","*","A","ME"]
[79,"ABBJ0230-","ZASUVKA REPRO STEREO BILA","KS",2,0,0,0,0,"S","*","A","ME"]
[80,0,"stropní držák projektoru","ks",1,0,0,0,0,"S","*","A","ME"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G100:G111)","v":0},null,null,null,null,null,null,"ME"]
[null,null,"Protipožární zařízen",null,null,null,null,null,null,null,null,"B","ME"]
[81,932,"ohnivzdorná přepážka s výplní(obecná položka)","m2",0.5,0,{"$f":"E114*F114","v":0},0,{"$f":"E114*H114","v":0},"S",null,"B","ME"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G114:G114)","v":0},null,null,null,null,null,null,"ME"]
[null,null,"součet",null,null,null,{"$f":"SUM(G24:G115)","v":0},null,{"$f":"SUM(I24:I115)","v":0}]
["Materiál zemní+stavební"]
[82,46134,"beton B13,5","m3",0.05,0,{"$f":"E118*F118","v":0},0,{"$f":"E118*H118","v":0},"S",null,null,"MZ"]
[83,46141,"malta vápenocementová","kg",110,0,{"$f":"E119*F119","v":0},0,{"$f":"E119*H119","v":0},"S",null,null,"MZ"]
[84,46181,"cihla vápenopísková 24/11,5/7,1","ks",103,0,{"$f":"E120*F120","v":0},0,{"$f":"E120*H120","v":0},"S",null,null,"MZ"]
[85,46231,"plech FeZn tl.0,5mm","m2",0.63,0,{"$f":"E121*F121","v":0},0,{"$f":"E121*H121","v":0},"S",null,null,"MZ"]
[null,null,"součet",null,null,null,{"$f":"SUM(G118:G121)","v":0},null,{"$f":"SUM(I118:I121)","v":0}]
["Elektromontáže"]
[null,null,"Kabely",null,null,null,null,null,null,null,null,"K","CE"]
[86,210800006,"vodič Cu(-CY) pod omítkou do 1x16","m",50,0,{"$f":"E125*F125","v":0},0,{"$f":"E125*H125","v":0},"S",null,"K","CE"]
[87,210800006,"vodič Cu(-CY) pod omítkou do 1x16","m",100,0,0,0,0,"S",null,"K","CE"]
[88,210800006,"vodič Cu(-CY) pod omítkou do 1x16","m",60,0,0,0,0,"S",null,"K","CE"]
[89,210800103,"kabel Cu(-CYKY) pod omítkou do 2x4/3x2,5/5x1,5","m",1500,0,0,0,0,"S",null,"K","CE"]
[90,210800103,"kabel Cu(-CYKY) pod omítkou do 2x4/3x2,5/5x1,5","m",200,0,0,0,0,"S",null,"K","CE"]
[91,210800103,"kabel Cu(-CYKY) pod omítkou do 2x4/3x2,5/5x1,5","m",2850,0,0,0,0,"S",null,"K","CE"]
[92,210800112,"kabel Cu(-CYKY) pod omítkou do 5x6","m",20,0,0,0,0,"S",null,"K","CE"]
[93,210800112,"kabel Cu(-CYKY) pod omítkou do 5x6","m",45,0,0,0,0,"S",null,"K","CE"]
[94,210800114,"kabel Cu(-CYKY) pod omítkou do 5x16","m",18,0,0,0,0,"S",null,"K","CE"]
[95,210810101,"kabel Cu(-1kV CYKY) pevně uložený do 3x35/4x25","m",22,0,0,0,0,"S",null,"K","CE"]
[96,210100001,"ukončení v rozvaděči vč.zapojení vodiče do 2,5mm2","ks",300,0,0,0,0,"S","*","K","CE"]
[97,210100002,"ukončení v rozvaděči vč.zapojení vodiče do 6mm2","ks",12,0,0,0,0,"S","*","K","CE"]
[98,210100003,"ukončení v rozvaděči vč.zapojení vodiče do 16mm2","ks",20,0,0,0,0,"S","*","K","CE"]
[99,210100004,"ukončení v rozvaděči vč.zapojení vodiče do 25mm2","ks",10,0,0,0,0,"S","*","K","CE"]
[100,210100007,"ukončení v rozvaděči vč.zapojení vodiče do 70mm2","ks",1,0,0,0,0,"S","*","K","CE"]
[101,210100003,"ukončení v rozvaděči vč.zapojení vodiče do 16mm2","ks",12,0,0,0,0,"S","*","K","CE"]
[102,210100004,"ukončení v rozvaděči vč.zapojení vodiče do 25mm2","ks",4,0,0,0,0,"S","*","K","CE"]
[103,210100007,"ukončení v rozvaděči vč.zapojení vodiče do 70mm2","ks",1,0,0,0,0,"S","*","K","CE"]
[104,210100009,"ukončení v rozvaděči vč.zapojení vodiče do 120mm2","ks",4,0,0,0,0,"S","*","K","CE"]
[105,210100012,"ukončení v rozvaděči vč.zapojení vodiče do 240mm2","ks",3,0,0,0,0,"S","*","K","CE"]
[106,210950101,"označovací štítek na kabel","ks",110,0,0,0,0,"S",null,"K","CE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G125:G145)","v":0},null,null,null,null,null,null,"CE"]
[null,null,"Materiál úložný",null,null,null,null,null,null,null,null,"M","CE"]
[107,210192562,"ochranná svorkovnice(nulový můstek)vč.zapoj.do 63A","ks",1,0,{"$f":"E148*F148","v":0},0,{"$f":"E148*H148","v":0},"S",null,"M","CE"]
[108,210010321,"krabicová rozvodka vč.svorkovn.a zapojení(-KR68)","ks",60,0,0,0,0,"S",null,"M","CE"]
[109,210010301,"krabice přístrojová bez zapojení","ks",100,0,0,0,0,"S",null,"M","CE"]
[110,210010301,"krabice přístrojová bez zapojení","ks",4,0,0,0,0,"S",null,"M","CE"]
[111,210010301,"krabice přístrojová bez zapojení","ks",76,0,0,0,0,"S",null,"M","CE"]
[112,210010301,"krabice přístrojová bez zapojení","ks",20,0,0,0,0,"S",null,"M","CE"]
[113,210010301,"krabice přístrojová bez zapojení","ks",54,0,0,0,0,"S",null,"M","CE"]
[114,210010301,"krabice přístrojová bez zapojení","ks",2,0,0,0,0,"S",null,"M","CE"]
[115,210010351,"krabicová rozvodka vč.ukonč.a zapojení (-6455/11)","ks",1,0,0,0,0,"S",null,"M","CE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G148:G156)","v":0},null,null,null,null,null,null,"CE"]
[null,null,"NNpřístroje",null,null,null,null,null,null,null,null,"N","CE"]
[116,210110081,"spínač 3pól/25A/400V(sporák přípoj)vč.zapoj nástěn","ks",1,0,{"$f":"E159*F159","v":0},0,{"$f":"E159*H159","v":0},"S",null,"N","CE"]
[117,210110041,"spínač zapuštěný vč.zapojení 1pólový/řazení 1","ks",20,0,0,0,0,"S",null,"N","CE"]
[118,210110045,"přepínač zapuštěný vč.zapojení střídavý/řazení 6","ks",4,0,0,0,0,"S",null,"N","CE"]
[119,210110043,"přepínač zapuštěný vč.zapojení sériový/řazení 5-5A","ks",18,0,0,0,0,"S",null,"N","CE"]
[120,210110064,"ovladač zapuštěný vč.zapojení tlačítkový/ř.1/0 S","ks",32,0,0,0,0,"S",null,"N","CE"]
[121,210110091,"spínač zapuštěný vč.zapojení s plynulou regulací","ks",1,0,0,0,0,"S",null,"N","CE"]
[122,210111012,"zásuvka domovní zapuštěná vč.zapojení průběžně","ks",30,0,0,0,0,"S",null,"N","CE"]
[123,210111012,"zásuvka domovní zapuštěná vč.zapojení průběžně","ks",435,0,0,0,0,"S",null,"N","CE"]
[124,210110091,"spínač zapuštěný vč.zapojení s plynulou regulací","ks",1,0,0,0,0,"S",null,"N","CE"]
[125,210150481,"relé časové vč.zapojení(-TX)","ks",2,0,0,0,0,"S",null,"N","CE"]
[126,210110064,"ovladač zapuštěný vč.zapojení tlačítkový/ř.1/0 S","ks",1,0,0,0,0,"S",null,"N","CE"]
[127,210110027,"spínač nástěnný od IP.2 vč.zapojení 3pólový/25A","ks",1,0,0,0,0,"S",null,"N","CE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G159:G170)","v":0},null,null,null,null,null,null,"CE"]
[null,null,"Osvětlení",null,null,null,null,null,null,null,null,"O","CE"]
[128,210201002,"svítidlo zářivkové bytové stropní/2 zdroje","ks",2,0,{"$f":"E173*F173","v":0},0,{"$f":"E173*H173","v":0},"S",null,"O","CE"]
[129,210201002,"svítidlo zářivkové bytové stropní/2 zdroje","ks",6,0,0,0,0,"S",null,"O","CE"]
[130,210200012,"svítidlo žárovkové bytové stropní/více zdrojů","ks",7,0,0,0,0,"S",null,"O","CE"]
[131,210200011,"svítidlo žárovkové bytové stropní/1 zdroj","ks",18,0,0,0,0,"S",null,"O","CE"]
[132,210202103,"E-svítidlo výbojkové venkovní na výložník","ks",1,0,0,0,0,"S",null,"O","CE"]
[133,210202103,"svítidlo výbojkové venkovní na výložník","ks",1,0,0,0,0,"S",null,"O","CE"]
[134,210201041,"svítidlo zářivkové nástěnné kompaktní","ks",1,0,0,0,0,"S",null,"O","CE"]
[135,210201041,"svítidlo zářivkové nástěnné kompaktní","ks",12,0,0,0,0,"S",null,"O","CE"]
[136,210200131,"svítidlo žárovkové průmyslové nástěnné","ks",2,0,0,0,0,"S",null,"O","CE"]
[137,210201002,"STÁVAJÍCÍ svítidlo zářivkové stropní/2 zdroje","ks",50,0,0,0,0,"S","*","O","CE"]
[138,210200041,"STÁVAJÍCÍ svítidlo žárovkové nástěnné/1 zdroj","ks",8,0,0,0,0,"S","*","O","CE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G173:G183)","v":0},null,null,null,null,null,null,"CE"]
[null,null,"Rozvaděče",null,null,null,null,null,null,null,null,"R","CE"]
[139,210191513,"kabelová skříň plast SPR2-SPR5 /osazení bez ukonč.","ks",1,0,{"$f":"E186*F186","v":0},0,{"$f":"E186*H186","v":0},"S",null,"R","CE"]
[140,210120103,"patrona nožové pojistky do 630A","ks",6,0,0,0,0,"S",null,"R","CE"]
[141,210120103,"patrona nožové pojistky do 630A","ks",3,0,0,0,0,"S",null,"R","CE"]
[142,210120103,"patrona nožové pojistky do 630A","ks",6,0,0,0,0,"S",null,"R","CE"]
[143,210120103,"patrona nožové pojistky do 630A","ks",3,0,0,0,0,"S",null,"R","CE"]
[144,210190002,"R1-rozvodnice do hmotnosti 50kg","ks",1,0,0,0,0,"S",null,"R","CE"]
[145,210190002,"R2-rozvodnice do hmotnosti 50kg","ks",1,0,0,0,0,"S","*","R","CE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G186:G192)","v":0},null,null,null,null,null,null,"CE"]
[null,null,"Slaboproud-místn.205",null,null,null,null,null,null,null,null,"A","CE"]
[146,210800103,"kabel Cu(-CYKY) pod omítkou do 2x4/3x2,5/5x1,5","m",70,0,{"$f":"E195*F195","v":0},0,{"$f":"E195*H195","v":0},"S",null,"A","CE"]
[147,210950341,"vodič/kabel v trubce jednotková hmotnost do 0,4kg","m",40,0,0,0,0,"S",null,"A","CE"]
[148,210111602,"zástrčka komunikační/konektor vč.zapojení 8pol","ks",1,0,0,0,0,"S",null,"A","CE"]
[149,210111312,"zásuvka domovní sdělovací 2násobná vč.zapojení","ks",1,0,0,0,0,"S",null,"A","CE"]
[150,210010002,"trubka plast ohebná,pod omítkou,typ 2316/pr.16","m",25,0,0,0,0,"S",null,"A","CE"]
[151,210020653,"nosná konstrukce přístroje do 50kg","ks",1,0,0,0,0,"S",null,"A","CE"]
[152,210200131,"svítidlo žárovkové průmyslové nástěnné","ks",4,0,0,0,0,"S",null,"A","CE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G195:G201)","v":0},null,null,null,null,null,null,"CE"]
[null,null,"Protipožární zařízen",null,null,null,null,null,null,null,null,"B","CE"]
[153,210020921,"ohnivzdorná přepážka s výplní ve stěně tl.15cm","m2",0.5,0,{"$f":"E204*F204","v":0},0,{"$f":"E204*H204","v":0},"S","*","B","CE"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G204:G204)","v":0},null,null,null,null,null,null,"CE"]
[null,null,"součet",null,null,null,{"$f":"SUM(G124:G205)","v":0},null,{"$f":"SUM(I124:I205)","v":0}]
["Zemní práce"]
[154,460270002,"OPRAVA zděný pilíř pro skříň SR","ks",1,0,{"$f":"E208*F208","v":0},0,{"$f":"E208*H208","v":0},"S","*",null,"CZ"]
[null,null,"součet",null,null,null,{"$f":"SUM(G208:G208)","v":0},null,{"$f":"SUM(I208:I208)","v":0}]
["Ostatní náklady"]
[155,219001233,"vybour.otvoru ve zdi/cihla/ do 0,09m2/tl.do 0,45m","ks",2,0,{"$f":"E211*F211","v":0},0,{"$f":"E211*H211","v":0},"S","*",null,"ON"]
[156,219003224,"zazdívka otvoru ve zdivu/cihla/do 0,09m2/tl.0,45m","ks",2,0,0,0,0,"S","*",null,"ON"]
[157,219001221,"vybour.otvoru ve zdi/cihla/ do 0,022m2/tl.do 0,15m","ks",40,0,0,0,0,"S","*",null,"ON"]
[158,219003212,"zazdívka otvoru ve zdivu/cihla/do 0,022m2/tl.0,15m","ks",40,0,0,0,0,"S","*",null,"ON"]
[159,219002271,"R1-vysekání výklenku/zeď cihla/ plocha od 0,25m2","m3",0.72,0,0,0,0,"S","*",null,"ON"]
[160,219003245,"R1-zazdívka otvoru ve zdivu/cihla/od 0,25m2 do 1,0","m3",0.72,0,0,0,0,"S","*",null,"ON"]
[161,219002271,"R2-vysekání výklenku/zeď cihla/ plocha od 0,25m2","m3",0.72,0,0,0,0,"S","*",null,"ON"]
[162,219003245,"R2-zazdívka otvoru ve zdivu/cihla/od 0,25m2 do 1,0","m3",0.72,0,0,0,0,"S","*",null,"ON"]
[163,219002611,"vysekání rýhy/zeď cihla/ hl.do 30mm/š.do 30mm","m",150,0,0,0,0,"S","*",null,"ON"]
[164,219003691,"omítka hladká rýhy ve stěně do 30mm vč.malty MV","m",150,0,0,0,0,"S","*",null,"ON"]
[165,219002631,"vysekání rýhy/zeď cihla/ hl.do 70mm/š.do 70mm","m",250,0,0,0,0,"S","*",null,"ON"]
[166,219003692,"omítka hladká rýhy ve stěně do 70mm vč.malty MV","m",250,0,0,0,0,"S","*",null,"ON"]
[167,219002641,"vysekání rýhy/zeď cihla/ hl.do 100mm/š.do 100mm","m",400,0,0,0,0,"S","*",null,"ON"]
[168,219003693,"omítka hladká rýhy ve stěně do 100mm vč.malty MV","m",400,0,0,0,0,"S","*",null,"ON"]
[169,219002661,"vysekání rýhy/zeď cihla/ hl.do 300mm/š.do 200mm","m",120,0,0,0,0,"S","*",null,"ON"]
[170,219003697,"omítka hladká rýhy ve stěně do 300mm vč.malty MV","m",120,0,0,0,0,"S","*",null,"ON"]
[171,219002671,"vysekání rýhy/zeď cihla/pod strop hl.30mm/š.30mm","m",220,0,0,0,0,"S","*",null,"ON"]
[172,219003591,"omítka hladká rýhy ve stropě do 30mm vč.malty MV","m",220,0,0,0,0,"S","*",null,"ON"]
[173,219990011,"Demontáže","hod",300,0,0,0,0,"S","*",null,"ON"]
[174,219990011,"Stěhování nábytku,úklid-25xkancel.á6hod.","hod",150,0,0,0,0,"S","*",null,"ON"]
[null,null,"Osvětlení",null,null,null,null,null,null,null,null,"O","ON"]
[175,218009001,"poplatek za recyklaci svítidla","ks",2,0,{"$f":"E232*F232","v":0},0,{"$f":"E232*H232","v":0},"Z",null,"O","ON"]
[176,218009011,"poplatek za recyklaci světelného zdroje","ks",4,0,0,0,0,"Z",null,"O","ON"]
[177,218009001,"poplatek za recyklaci svítidla","ks",6,0,0,0,0,"Z",null,"O","ON"]
[178,218009011,"poplatek za recyklaci světelného zdroje","ks",12,0,0,0,0,"Z",null,"O","ON"]
[179,218009001,"poplatek za recyklaci svítidla","ks",1,0,0,0,0,"Z",null,"O","ON"]
[180,218009011,"poplatek za recyklaci světelného zdroje","ks",1,0,0,0,0,"Z",null,"O","ON"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G232:G237)","v":0},null,null,null,null,null,null,"ON"]
[null,null,"součet",null,null,null,{"$f":"SUM(G211:G238)","v":0},null,{"$f":"SUM(I211:I238)","v":0}]
["Ochranné a pracovní pomůcky"]
[null,null,"Rozvaděče",null,null,null,null,null,null,null,null,"R","OP"]
[181,1031,"držák pojistek D1PH","ks",1,0,{"$f":"E242*F242","v":0},0,{"$f":"E242*H242","v":0},"S",null,"R","OP"]
[null,null,"                                        dílčí součet ",null,null,{"$f":"SUM(G242:G242)","v":0},null,null,null,null,null,null,"OP"]
[null,null,"součet",null,null,null,{"$f":"SUM(G241:G243)","v":0},null,{"$f":"SUM(I241:I243)","v":0}]
["Revize"]
[182,217309013,"vypracování zprávy VR/cena akce do 1.000.000 kč","ks",2,0,{"$f":"E246*F246","v":0},0,{"$f":"E246*H246","v":0},"Z","*",null,"RE"]
[null,null,"součet",null,null,null,{"$f":"SUM(G246:G246)","v":0},null,{"$f":"SUM(I246:I246)","v":0}]
[]
["Datum: 8.11.2016"]
["Vypracoval:"]